i-PRO WV-S8544 MULTI-SENSOR NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd 

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-S8544 MULTI-SENSOR NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Multi-Sensor Camera shall deliver H.265 stream and H.264 stream.

2.	The Multi-Sensor Camera shall utilize an approximate 1/2.8 type high sensitivity CMOS image sensor. 

3.	The Multi-Sensor Camera shall have four 4MP image sensors and produce a resolution of 2688 x 1520 pixels at up to 30 fps with a 16:9 aspect ratio. 

4.	The Multi-Sensor Camera shall built-in AI engine to enable analytical applications on network edge. Built-in AI engine supports the detecting suspicious changes in captured scenes, optimizing the image settings of the camera (based on captured scene analysis) for better image usability, and optimizing video compression through captured scenes to save bandwidth.

5.	The Multi-Sensor Camera shall enables to install the optional analytics applications with including developed by third party companies using this camera's SDK.

6.	The Multi-Sensor Camera shall have the four repositionable lenses with easy adjustment include a wide range tilt angle (+ 10 degrees to +105 degree) mechanism minimizes blind spots. 

7.	The Multi-Sensor Camera shall have Continuous view assistance feature which is automatically adjusts the angle of view of each horizontally aligned camera to reduce the overlap of images from each camera.

8.	The Multi-Sensor Camera shall feature a 102dB wide dynamic range based on Enhanced Super Dynamic and built-in AI engine and Adaptive Black Stretch technology (ABS). 

9.	The Multi-Sensor Camera shall produce a color image with a minimum illumination of 0.21 lux and a monochrome image with 0.12lux at F2.0, shutter speed of 1/30s.

10.	The Multi-Sensor Camera shall generate multiple simultaneous video streams of up to two (2) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams per camera.

11.	The Multi-Sensor Camera shall be equipped with AI intelligent auto mode which is the technology for shooting license plate and person’s face more clearly.

12.	The Multi-Sensor Camera shall be equipped with GOP controls including smart facial coding and frame control and it reduce bit rate by controlling the image quality of still areas, moving areas, and faces with AI engine.

13.	The Multi-Sensor Camera shall be equipped with corridor mode enables the capture of a more vertically-oriented area than the normal format would allow 

14.	The Multi-Sensor Camera shall produce encrypted stream.

15.	The Multi-Sensor Camera shall realize SSL / TLS communication with CA certificate. 

16.	The Multi-Sensor Camera shall realize a high level of cyber security with FIPS 140-2 level3 certified hardware.

17.	The Multi-Sensor Camera shall be rated to IK10 vandal resistance

18.	The Multi-Sensor Camera shall be rated to IP67/IP66 and NEMA 4X standard against water and dust ingress

19.	A user shall be able to view video on a PC using a browser.

20.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

21.	The Multi-Sensor Camera shall offer Video Motion Detection (VMD) with four (4) per camera programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

22.	The Multi-Sensor Camera shall offer Scene Change Detection (SCD) is possible to issue an alarm when a camera is covered with something or the camera direction is changed to shoot a different subject.

23.	The Multi-Sensor Camera shall have Fog compensation function.

24.	The Multi-Sensor Camera shall have High light compensation (HLC) function.

25.	The Multi-Sensor Camera shall have Super Chroma Compensation (SCC) which realizes a better color reproducibility in the low illumination.

26.	The Multi-Sensor Camera shall provide up to eight (8) areas of electronic privacy masking per camera. 

27.	The multi-sensor camera shall have a USB terminal for confirming the live image and adjusting viewing angle with the smartphone or tablet device via the Wi-Fi connection at installation. 

28.	The Multi-Sensor Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

29.	The Multi-Sensor Camera shall have a micro SD memory card slot that supports micro SDXC memory card for local storage. 

30.	The Multi-Sensor Camera shall offer full-duplex bi-directional audio communication capability between the camera and monitoring site.

31.	The Multi-Sensor Camera shall have three (3) alarm sources of terminal input, VMD, SCD, command alarm , and audio detection alarm that activate the processes such as micro SDXC memory recording, E-mail notification, HTTP alarm notification, Indication on browser, and Panasonic alarm protocol output.

32.	The Multi-Sensor Camera shall conform to the ONVIF Profile. 

B.	CAMERA
1.	Image Sensor		4 x 1/2.8 type CMOS image sensor
2.	Effective Pixels                    Approx. 16mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.21 lux (30IRE, F2.0, Maximum shutter: Off(1/30s), AGC: 11)
0.3 lux (50IRE, F2.0, Maximum shutter: Off(1/30s), AGC: 11)
b.	B/W			0.12 lux (50IRE, F2.0, Maximum shutter: Off(1/30s), AGC: 11)
5.	Day & Night		IR Cut filter Removal
6.	Dynamic Range		102 dB typ. (Super Dynamic: On)
             7． Image Rotation		0°/ 90°/ 180°/ 270°
             8.    Video Analytics
	a. AI Video Motion Detection	WV-XAE200W
b. AI Non-Mask Detection               WV-XAE203W
c. AI Face Detection                        WV-XAE204W (Max. 2ch)
d. AI People Detection                     WV-XAE205W
e. AI Vehicle Detection                    WV-XAE206W
f. AI Occupancy Detection               WV-XAE207W
g. Upload App Capability / Third-party applications
With AI engine to enable to install and activate up to four video analytical application

C.	Lens
1.	Focal Length		2.9-7.3 mm
2.	Optical Zoom		2.5x
3.	with Extra Zoom @640x360 10.5x
4.	Zoom Control		Motorized
5.	Focus Adjustment		Auto Focus
6.	Aperture Ratio		F2.0-F3.0
7.	Angular Field of View
a.	16:9 aspect ratio	H: 43-100°
V: 24-56°
             8.     Adjusting Angle                 
                       a.      Camera　　　         Horizontal (PAN) angle : ±125  °,Twist: ±20 °
Vertical (TILT) angle     : +10 ° to +105 °
Azimuth (YAW) angle   : ±90 °

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG

2.	Image Resolution
a.	16:9 aspect ratio
2688x1520, 2560x1440, 1920x1080, 1280x720, 640x360, 320x180 

3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate / VBR / Frame rate / Best effort
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 30 fps (30 fps mode)
                                  1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 fps (12.5 fps mode)
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1024 / 1536 / 2048 / 3072 / 
4096 / 6144 / 8192 / 10240 / 12288 / 14336 / 16384 kbps
--FREE ENTRY--
d.	Image Quality	
i.	Constant bit rate	Low (Motion priority) / Normal / Fine (Image quality priority)
ii.	Frame rate           Low (Motion priority) / Normal / Fine (Image quality priority)
iii.	Best effort	Low (Motion priority) / Normal / Fine (Image quality priority)
iv.	VBR		10 steps
e.	Transmission type	Unicast port(AUTO) / Unicast port(MANUAL) / Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push
5.	Smart Coding
a.	GOP(Group of picture) control
Off/ Low (Variable GOP 1s-8s)/ Mid (Variable GOP 4s-16s)
/Advanced (Fixed GOP 60 seconds with 1 second Key frame)
/Frame rate control (Variable GOP 4s-16s with frame rate control)
*Advanced and Frame rate control are only available with H.265.
b.	Smart VIQS			On(High)/On(Low)/Off
c.	Smart P-picture control	On/Off

E.	Audio
a.	Audio Compression	G.726 (ADPCM) 32kbps / 16kbps, G.711 64kbps, 
AAC-LC 128 / 96 /  64 kbps
b.	Audio Mode		OFF / Mic(Line) input /output/ Interactive (Half duplex) /
                                   Interactive (Full duplex)

F.	OPERATION
1.	Super Dynamic		On / Off
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
4.	Fog compensation		On / Off The level can be set in the range of 0 to 8 
(Only when intelligent auto / auto contrast adjust: Off)
5.	Back light compensation
High light compensation	BLC (Back light compensation) / HLC (High light compensation) /
Off  
The level can be set in the range of 0 to 31
 (Only when Super dynamic and intelligent Auto is off)
6.	AGC			The level can be set in the range of 0 to 11.
7.	Shutter Speed		1/10000 to 16/30 s (30fps mode)
1/10000 to 16/25 s (25fps mode)
8.	Day & Night		Off / On / Auto1 (Normal) / Auto2 (IR Light) / Auto3 (SCC)
9.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
10.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps
11.	Scene Change Detection(SCD)  On / Off, 1 area
12.	Audio Detection	            On / Off
13.	AI Sound Classification       Gunshot, Yell, Vehicle horn, Glass break
14.	Privacy Zone		On / Off, Up to 8 zones
15.	Camera Title (OSD)	40 characters
16.	Image overlay		Yes
17.	Digital Zoom		x1, x2, x4

G.	NETWORK
1.	Network Interface		10BASE-T / 100BASE-TX / 1000Base-T, RJ-45 connector
2.	IP				IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, SMTP, DNS, NTP,
SNMPv1/v2/v3, DHCPv6, RTP, MLD, ICMP, ARP,
IEEE 802.1X, DiffServ, LLDP
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, RTSP, RTP,
RTP/RTCP, SMTP, DHCP, DNS, DDNS, NTP, SNMPv1/v2/v3,
UPnP, IGMP, ICMP, ARP, IEEE 802.1X, DiffServ, SRTP, LLDP 
4.	Max. User access		Up to 24 users
5.	Mobile Terminal Compatibility
iPad, iPhone, AndroidTM mobile terminals
6.	ONVIF®*			Profile G/M/S/T (T.B.D)
*ONVIF is a trademark of ONVIF,Inc.

H.	INTERFACE
1.	Monitor Output		USB terminal via Wi-Fi connection
2.	Microphone input / Line input
				ø3.5 mm stereo mini jack
3.	Audio Output		ø3.5 mm stereo mini jack (monaural output)
4.	External I/O Terminals	ALARM IN 1 (Alarm input 1/ DayNight input/
Auto time adjustment input) (x1)
 ALARM IN 2 (Alarm input 2/ ALARM OUT) (x1)
ALARM IN 3 (Alarm input 3/ ALARM OUT /AUX OUT) (x1)
5.	SD memory card slot	1 slot, micro SDXC

I.	ELECTRICAL
1.	Power Source		PoE+(IEEE802.3at)
2.	Power Consumption	PoE+: 470mA/25.5W (T.B.D) (class 4)
3.	

J.	SAFETY / EMC
1.	Safety			UL (UL60950-1), c-UL (CSA C22.2 No.60950-1), CE, IEC60950-1
2.	EMC 			FCC (Part15 Class A), ICES003 Class A, EN55032 Class B, 
				EN55024

K.	MECHANICAL
1.	Dimensions 		ø300 mm × 90 mm (H)(T.B.D)
                                           * When using attachment plate only
2.	Weight			Approx. 3.5kg (T.B.D)　
3.	Construction material
a.	Main body		Aluminum die cast
b.	Outer fixing screws   Stemless steel (Corrosion-resistant treatment)
c.	Dome cover		Polycarbonate resin
4.	Finish
a.	Main body		i-PRO white
b.	Dome cover		Clear

L.	ENVIRONMENTAL
1.	Ingress Resistance	IP67/IP66 (IEC60529), NEMA 4X compliant 
2.	Vandal Resistance	IK10 (IEC 62262)
3.	Wind Resistance               Up to 40 m/s {approx. 89 mph}
4.	Operating Temperature	-40 °C ~ +60 °C (-40 °F ~ 140 °F)
 (Power On range: –20 °C to +60 °C {–4 °F to 140 °F})
5.	Operating Humidity	 10 % ~ 100 % (without condensation)

M.	Other Functions
1.	Wide range tilt angle adjustment mechanism
2.	Intelligent Auto(with AI)
3.	Easy Kitting Package
4.	Continuous view assistance
5.	Simple Stitching Mode / Quad Mode
6.	NEMA TS2 (T.B.D)

N.	Options
1.	Dome Cover		WV-QDC501G
2.	Cable			WV-QCA500A/WV-QCA500APK
				WV-QCA501A/WV-QCA501APK